RFP-2SH8 Cold Box Conversion Addendum 4 3/27/25

**QUESTION:**

Can we get lintel requirements for the holes being cut in the block walls? Lintels are typically required for opening above a certain size. May not be needed for these sizes but want to confirm.

**L3HARRIS RESPONSE:**

The opening that you reference already exists. Please refer to Sheet G-001 and Sheet AD 102.