RFP-2SH8 Cold Box Conversion Addendum 9 3/31/25

**QUESTION:**

What kind of access control for the new buildings and renovations.

**L3HARRIS RESPONSE: (see attached manual)**

VANDERBILT hardware must be installed by VANDERBILT certified installers.

Currently we use Triple-S and Convergint for installations.

Standard builds for us here in Camden

Vanderbilt Panels VRCNX-A , panel expandable to 16 readers through up to 8 VRI-2SH downstream panels.

VRI-2S3 downstream reader panels/2 readers per panel

HID readers HID multiclass SE RK40

Strikes any functional on 12-24V