**Kinco Bid Manual**

**SECTION 3: SCOPE OF WORK**

**BID PACKAGE 05 13 – STRUCTURAL STEEL SUPPLY**

Your signature on this page is a confirmation of your bid and an acknowledgement and acceptance of the requirements of the Kinco Bid Manual, project schedule and all Addendums and CM Clarifications.

Company AR State Contractor’s License #

Name Title

Address

City State Zip Code

Phone Number w/ Area Code Email Address

**Specification:**

Bidders will include work from referenced specifications and other work normally associated with this trade whether referenced or not.

**Scope of Work:**

The bid package shall also include the following items but shall not limit more stringent requirements found elsewhere in the contract documents unless specifically listed as exclusion below.

1. Contractor shall furnish all PEMB structural and misc. steel including the following but not limited to: embed plates, pour stop angles, support plates, steel decking, x-bracing, bent plates, C-channels, bar joists, tube steel, columns, beams, steel stairs, bridging, masonry steel lintels, closure angles, pipe bollards, interior and exterior guard and wall rails, hand rails, hand rail embed sleeves.
2. Contractor shall furnish all misc. steel for elevator including, pit ladder, sump pump grate, embed angles, hoist beam, support columns for rails.
3. Contractor to furnish all steel at kitchen exhaust pit including but not limited to the pit ladder, metal grate, hinged access door, metal cap, C-channels.
4. Supply all required anchor bolts for structural steel to be installed by concrete contractor.
5. Contractor shall furnish all architectural and miscellaneous steel per all the Contract Documents and as required for a complete installation.
6. Contractor shall furnish all fasteners and attachments (bolts, screws, threaded rods, erection bolts, washers, torque nuts, expansion anchors, stud anchors, lag bolts, steel shims, nelson studs etc.) as required for a complete erection of this bid package.
7. Contractor shall furnish all galvanizing or electroplating that is required by the Contract Documents.
8. Contractor shall supply manufacturer’s data and samples, certifications for connections of structural steel members, and welding certificates.
9. Contractor shall include any special preparation of architecturally exposed steel.
10. Deliver shortages of fabricator errors within 24 hours of notification.
11. The shipment shall be properly bundled, packaged, and palletized. Contractor shall furnish adequate dunnage for on-site storage. Material shall be free and clean from dirt.
12. Include all state and local sales tax.
13. Contractor shall furnish and install primers for steel that is to receive an architectural finish.
14. Contractor shall furnish any support steel for counter tops, light fixtures, etc. as shown on the Contract
15. Contractor shall furnish all required miscellaneous metal supports, stands, hangers, etc. required for all mechanical equipment that are specifically shown and sized on the Structural Drawings, both permanent and temporary.
16. The shipment shall be properly bundled, packaged, and palletized with piece marks clearly visible for proper erection. Contractor shall furnish adequate dunnage for on-site storage. Material shall be free and clean from dirt.
17. Contractor is to deliver shortages of fabricator errors within 24 hours of notification.
18. Contractor to meet all project specified sustainability requirement.

|  |  |
| --- | --- |
| **BASE BID to provide materials, including all taxes, as****required by this bid package and listed specifications.** | **$**  |

|  |
| --- |
| **ALTERNATE #1 –**  |
|  | **$** |

VOLUNTARY VALUE ANALYSIS

Value Analysis propositions will be strongly considered in the subcontractor selection process. Bidders are encouraged to explore and identify Value Analysis savings for this scope of work. Please describe below (and on separate page if necessary) any cost saving opportunities as well as potential savings:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Bidder acknowledges receipt of the following addenda:

1. Dated:
2. Dated:
3. Dated:

Bidder acknowledges receipt of the following CM Clarifications:

1. Dated:
2. Dated:
3. Dated: